;
LanguageName=
;
;
0000="&File",
0001="E&xit",
0002="Exit the application",
0003="Error",
0004="Language Update Failed",
0005="&Open",
0006="Load binary file",
0007="&Save",
0008="Save data for backup",
0009="&Tools",
0010="Config",
0011="Configure the target",
0012="Detect Chip (F1)",
0013="Detect chip ID",
0014="Read from chip (F2)",
0015="Read data from target",
0016="Verify data (F3)",
0017="Verify the data between memory and target",
0018="Erase chip (F4)",
0019="Erase the memory block on the chip",
0020="Write chip (CTRL+W)",
0021="Write data to target chip",
0022="Activation",
0023="Activate the software based on hardware ID",
0024="New Flash",
0025="Enter new flash type to flash.xml",
0026="New Target XML",
0027="Create new target test xml",
0028="&Help",
0029="&About",
0030="About USBJTAG NT ....",
0031="Connection",
0032="Show connection diagram",
0033="Goto Configure folder",
0034="Open configuration folder",
0035=" Range: ",
0036="   Speed: ",
0037="Test Module Not Loaded",
0038="No Hardware",
0039="Category",
0040="Target select",
0041="Register View",
0042="Auto Script",
0043="Script Directory",
0044="Select Script Directory",
0045="Add Flash Type",
0046="CopyFrom",
0047="Number of Sector",
0048="Sector Size",
0049="Name",
0050="Size",
0051="Type",
0052="SPI flash",
0053="Name conflict",
0054="Size Error",
0055="Type(0-RAM, 1-Flash,\n 2-EEPROM,3-NAND)",
0056="Start Address",
0057="Protocol",
0058="No",
0059="Yes",
0060="IR Length",
0061="Program Memory",
0062="Memory definitions",
0063="Address",
0064="New",
0065="Clear",
0066="View XML",
0067="Duplicate Test Name",
0068="Email Activate",
0069="Online Activation",
0070="Hardware ID",
0071="Email Address",
0072="Activation Code",
0073="Please enter your Paypal email address",
0074="Network Error",
0075="Disconnected",
0076="USB connected",
0077="IRLength is out of range, use default 5",
0078="Target: ",
0079="Warning!!",
0080="Are you sure you want to program?  ",
0081="Are you sure you want to erase?  ",
0082="Erase time",
0083="Program time",
0084="Peeked Address",
0085="Found Address",
0086="Unknown flash type!",
0087="Report these values",
0088="Read speed",
0089="Compare data Failed address",
0090="Check memory range.",
0091="Time",
0092="Save binary file",
0093="Compare data OK",
0094="Bus Error!",
0095="Command unknown ",
0096="Note this is 64bit MIPS,Please fix the  xml file",
0097="Note this is not 64bit MIPS,Please fix the  xml file",
0098="DMA supported",
0099="DMA not supported",
0100="Write speed",
0101="Program speed",
0102="Program pass, if no further programming needed, power off/on the target",
0103="Program Starts...",
0104="Flash blanked",
0105="Flash is not blank at address",
0106="Hardware incompatible",
0107="Busy",
0108="EepomRegAddr is not defined in xml",
0109="Not finished last program",
0110="Detect the flash type first!",
0111="Not a flash area",
0112="Flash protocol not supported",
0113="Dest must start at the boundary of a block",
0114="Check your configuration or detect the flash first",
0115="Erase starts...",
0116="Address or size should be on the boundary of a flash",
0117="Already in debug mode",
0118="AllFlash",
0119="Output",
0120="Copy",
0121="Copy the current selection's contents to the clipboard",
0122="Paste",
0123="Paste the clipboard's contents into the current position",
0124="Init",
0125="Fill the memory tab with initial value",
0126="Usage: init\r\n Initialize the target So memories are accessible",
0127="Usage: initusb\r\n Reinit the USB port.",
0128="Usage: exit\r\n Exit the application.",
0129="Usage: help (cmd)\r\n Output the usage of the command.",
0130="Usage: reset\r\n Reset the device. Send reset signal. For BDM param=1 will enable BDM.",
0131="Usage: detect\r\n Detect the JTAG devices.",
0132="Usage: search start end step\r\n Search memory from start to end with step",
0133="Usage: peek address\r\n Get the word data of a memory",
0134="Usage: poke address data\r\n Set the word data of a memory",
0135="Usage:getram address length\r\n Usage:getram tabname\r\n Get the memory from target to PC memory",
0136="Usage:cmpram address length\r\n Usage:cmpram tabname\r\n compare memory between target and PC memory",
0137="Usage:setram address length\r\n Usage:setram tabname\r\n Set the memory to target from PC memory",
0138="Usage: save tabname (filename)\r\n save start end (filename)\r\n Save the data in the tab",
0139="Usage:ldram address (filename)\r\n Usage:ldram tabname\r\n Load memory.",
0140="Address out of range",
0141="Usage: program address length\r\n Usage program tabname\r\n program flash.",
0142="Can not find the memory in the configuration",
0143="Usage: flshlist (type)\r\nList all the flash types (nor,spi,nand,spinand)",
0144="Supported flash type list:",
0145="Usage: flshdct (address)\r\nDetect flash chip,",
0146="Usage: d address.\r\n Make the address visible",
0147="Configure the memory map",
0148="Usage: about\r\n Display version info",
0149="Usage: cls\r\n Clear the output display",
0150="Usage: e address data data ....\r\n Edit address with new data.",
0151="Usage: f tabname(address length) data\r\n Fill with new data.",
0152="Usage: s tabname(address length) string (data data data)\r\n t Search for data or string.\r\n eg. s nvram ASTB\r\n eg: s 210000 2000 22 33 44 55",
0153="Not Found",
0154="Usage: configshow\r\nShow Existing config.",
0155="Config file error!",
0156="No configuration",
0157="Usage: erase address length\r\n Usage:erasem tabname\r\n Erase the flash",
0158="Usage: flshset tabname value1,value2\r\nForce flash setting to tabs,",
0159="Usage: sprogram address length\r\n Usage:sprogram tabname\r\n Slow program flash (must erase first)",
0160="Usage: bk\r\n Break the target",
0161="Usage: r (regname value)\r\n read/set register value",
0162="Register not valid",
0163="Register can not be set",
0164="Usage: t\r\n Single step",
0165="Step can not exceed 65536",
0166="Not in debug mode",
0167="Usage: t= address\r\n Single step with address.\r\n t= 468",
0168="Usage: g\r\n Continue excute.",
0169="Usage:g= address \r\n Excute at address",
0170="Usage: pokeh address data\r\n Poke half word",
0171="Usage: pokeb address data\r\n Poke byte",
0172="Usage: blkchk address length\r\n Usage:blkchk tabname\r\n Blank check flash",
0173="Usage: flshdcth (address)\r\nDetect flash chip in half word",
0174="Usage:ldramh address (filename)\r\n Load memory in half word.",
0175="Usage: speed 0 (1) (2)\r\nAdjust target speed 0 fast, 1 middle,2 slow",
0176="Usage: cfi (1) 0\r\n Enable/disable the CFI.",
0177="Usage: log (1) 0\r\n Enable/disable the log.",
0178="Usage:sgetram address length\r\n Usage:getram tabname\r\n Get the memory from target to PC memory use slow mode",
0179="Usage:scmpram address length\r\n Usage:cmpram tabname\r\n compare memory between target and PC memory using slow mode.",
0180="Usage:setram address length\r\n Usage:setram tabname\r\n Set the memory to target from PC memory using slow mode",
0181="Usage: ldhex \r\n Load memory from hex file.",
0182="Usage: sphex \r\n Slow program hex file.",
0183="Usage: prhex \r\nprogram hex file.",
0184="Usage: peekh address\r\n Peek half word",
0185="Usage: peekb address\r\n Peek byte",
0186="Usage: color ffffff\r\n Change back ground color",
0187="Usage: script \r\nDisplay all the script files\r\n script file\r\n Display script",
0188="Script file error!",
0189="No script files",
0190="Usage:BL \r\nList current break points",
0191="Usage: be n\r\n Usage: be *\r\n Enable one (or all) break point",
0192="Usage: bd n\r\n Usage: bd *\r\n Disable one (or all) break point",
0193="Usage: bpm address\r\n Break on memory address",
0194="Usage: bpx address\r\n Break on code address",
0195="Please select",
0196="Please select right value",
0197="Exit Script",
0198="Press enter to continue.Spacebar and enter to break....",
0199="Bad command",
0200="Script finished",
0201="Clear command window",
0202="Language",
0203="Select new language",
0204="Language Selection",
0205="Available Language",
0206="Usage: fullprac 0/1 disable or enable full prac",
0207="Usage: pgmram address set program ram",
0208="Usage: JAM command (eg. JAM PROGRAM)",
0209="Usage: config (target)",
0210="loaded",
0211="File Error",
0212="Saved",
0213="Wrong target selected",
0214="&Recent Files",
0215="&Recent Targets",
0216="Not Activated",
0217="Activated",
0218="Clear output window",
0219="Usage:REGS 1(0) \r\nDisplay (hide) internal registers after CPUID",
0220="Target incompatible",
0221="Search Target For",
0222="Edit Device File",
0223="Please wait...",
0224="Split",
0225="Target not exist",
0226="Not enough data",
0227="Import Target XML",
0228="Usage:POWER 1(0) \r\nControl power on/off the target (relay)",
0229="General",
0230="File Save Option",
0231="Auto Save After Read",
0232="File name",
0233="Flash",
0234="Date",
0235="Tab Name",
0236="Blank Check",
0237="Check if flash is blanked",
0238="Password",
0239="Record",
0240="Stop",
0241="Auto Verify After Program",
0242="Find",
0243="Find Next",
0244="Replace",
0245="Calculate checksum",
0246="Ignore using checksum to compare",
END
